**SHORT DESCRIPTION OF THE WORK TO BE DONE FOR THE ROAD REHABILITATION OF GOBWEYN FARM ACCESS ROAD**

1. **Road Widening, Leveling, Watering, and Compaction with front loader or greder:** The 1.7km road will be expanded to a width of 6 meters. This process involves excavating the current terrain and adding soil as needed to reach the required width. After widening, the road will be leveled to create a smooth and even surface. The cut and fill technique will be applied to achieve the necessary elevation. The leveled surface will then be watered and compacted using rollers or compactors, ensuring a stable and durable foundation for the road.
2. **Murrum Soil Laying:** After the road surface has been prepared, a 15cm thick layer of murrum soil will be laid and compacted over the rough 1.7km stretch indicated by the red line. Murrum soil is chosen for its stability and durability in road construction.